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	EHS COMMUNITY
Confined Space Entry Permit
Per 29 CFR 1910.146 — Permit-Required Confined Spaces



	Permit #



	⚠ PERMIT-REQUIRED CONFINED SPACE ENTRY. This permit must be completed and signed by the Entry Supervisor before any entrant enters the space. The permit is valid only for the date and duration listed. Cancel immediately if conditions change or the job scope changes.



	SECTION 1 — SPACE & JOB IDENTIFICATION



	Space Name / Location
	Space Description / ID
	Purpose of Entry



	Permit Date
	Valid From (Time)
	Permit Expires (Time)
	Maximum # Entrants



	SECTION 2 — HAZARDS PRESENT IN THIS SPACE



	Potential Hazard
	Present? (Y/N)
	Control Measure

	Oxygen-deficient atmosphere (<19.5%)
	
	

	Oxygen-enriched atmosphere (>23.5%)
	
	

	Flammable gas / vapor (>10% LEL)
	
	

	Toxic air contaminant (above PEL)
	
	

	Engulfment / flooding hazard
	
	

	Internal configuration / entrapment
	
	

	Mechanical / energized equipment
	
	

	Thermal (heat / cold stress)
	
	

	Other: _______________________
	
	



	SECTION 3 — ATMOSPHERIC TESTING LOG



Before entry, test in this order: oxygen, then combustible gases and vapors, then toxic gases and vapors (29 CFR 1910.146(d)(5)(iii)). During entry, test or monitor as often as needed to confirm acceptable conditions are maintained (d)(5)(ii); monitor continuously where the space cannot be isolated (d)(5)(i). Continuous monitoring, and testing at several levels where the atmosphere may be stratified (Appendix B to 1910.146), are good practice. Column limits are US federal OSHA values; Cal/OSHA's are lower (8 CCR 5155: CO 25 ppm and H₂S 10 ppm 8-hour PELs) and Canadian provinces set their own, so use the limits for your jurisdiction.
	Time
	Tested By
	Instrument / Cal. Date
	O₂ % (19.5–23.5%)
	LEL % (<10%)
	CO ppm (US PEL: 50, 8-hr TWA)
	H₂S ppm (US ceiling: 20)
	Other
	Safe to Enter?

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	



	SECTION 4 — ISOLATION & ENERGY CONTROL



	LOTO Procedure # / Equipment Isolated
	Lines Blanked / Blinded
	Ventilation Provided (Type / CFM)



	SECTION 5 — REQUIRED PPE



	Respiratory Protection
	Retrieval / Rescue Equipment
	Other PPE Required



	SECTION 6 — PERSONNEL



	Role
	Name (Print)
	Signature
	Time In
	Time Out

	Entry Supervisor
	
	
	—
	—

	Attendant (Outside)
	
	
	—
	—

	Authorized Entrant 1
	
	
	
	

	Authorized Entrant 2
	
	
	
	

	Rescue Service Contact
	
	—
	—
	—



	Rescue Service Phone
	



	SECTION 7 — RESCUE PLAN



	Non-Entry Rescue Method (preferred)
	Emergency Contact / 911 Access Point



	PERMIT CANCELLATION / CLOSURE



	Reason for Cancellation or Completion
	Cancelled / Closed By
	Time



Cancelled permits must be retained for at least 1 year per 29 CFR 1910.146(e)(6) so that failures can be reviewed during the annual review of the confined space program.
This template is provided for educational purposes by EHS Community (ehscommunity.com). It does not constitute legal advice. Reference: 29 CFR 1910.146 — Permit-Required Confined Spaces.
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